Recent Changes - Search:

Information Foreword What is EJS? Demos/Examples Credits Links Webcasts Installation Download & Install EJS Workspaces Running EJS Conditions of Use Documentation EJS Console EJS Interface Description Panel Model Panel View Panel Deployment Elements Reference User Feedback English | Spanish | ? View Edit History Print PDF ## Transmission line The simulation program TL (Transmission Line) is based on solutions of Maxwell´s equations in one dimension, the so-called transmission line equations. The algorithm was developed originally by Zvonko Fazarinc with later additions by Ernesto Martín, and has been proven to be stable and correct for all possible border conditions and parameter settings. The program TL can be applied primarily to visualize dynamic processes on a double line with superposition and reflection as basic concepts. This is useful not only for ac and high frequency systems but also for dc-currents when the focus is set on transition processes, linking different stationary states, determined by Ohm´s law and Kirchhoff´s laws. Click on the image to start the applet. Applet ‘TeEl’. Download the self-executable JAR file or a ZIP file with the XML source code for this example. To inspect and run the example, you will need to have EJS installed in your computer (see Installation), uncompress the downloaded ZIP file anywhere in the source directory of your EJS workspace and load it with EJS.

Edit - History - Print - Recent Changes - Search
Page last modified on June 01, 2009, at 09:29 PM